                        Orchid Technology 
               Fahrenheit 64 and Fahrenheit Pro 64
                      Driver Release v1.22
             ---------------------------------------

The file you have downloaded, !F64.EXE contains the complete 
files from the Fahrenheit Install/Driver disk v1.22.  This readme 
file contains instructions for making a Fahrenheit driver disk, 
so you can install the drivers.  You have already completed the 
first step, by unpacking the !F64.EXE file and reading this.  

When you unpack !F64.EXE you should have the following files:


FAH64    001   1044164 03-27-95   1:22a
INSTALL  EXE    179498 03-22-95   1:22a
SETUP    EXE    229284 03-22-95   1:22a
README   1ST      3415 08-03-95   


Using your Fahrenheit Drivers
-----------------------------
There are two ways to install the Fahrenheit software drivers and 
utilities.  You can install the software to your hard drive 
through Windows or DOS.  Both installation programs are the same; 
use the one most convenient for you.  For brevity only the DOS 
installation is covered in this readme file.  For instructions on 
the Windows installation, see your Fahrenheit manual.

1.  Copy all files (listed above) to a blank high density 3.5" 
    floppy disk.

2.  Log onto your floppy drive and run the INSTALL.EXE program          
    install the driver files to your hard drive.  You should run 
    INSTALL.EXE from DOS, not from Windows.

The INSTALL.EXE program is menu driven, and fairly self 
explanatory.  The INSTALL menu helps you install drivers for a 
variety of different applications.  If you have questions during 
any part of the installation process, press the F1 key for 
context sensitive help, or see your Fahrenheit manual for more 
information.


Troubleshooting
---------------
If you're using QEMM or EMM386 (or a similar type of memory 
manager),  you need to exclude the Fahrenheit's RAM and ROM 
memory address so your memory manager doesn't try to use that 
area.  The syntax for EMM386 and QEMM is to add the statement  
X=A000-C7FF  to the EMM or QEMM setup line in your CONFIG.SYS 
file.  If you are using QEMM's "Stealth" feature (ST:M or ST:F), 
you also need to add the statement XST=C000 to the QEMM line in 
CONFIG.SYS.  If you use QEMM, it may be necessary to re-run the 
Optimize program after adding the Fahrenheit exclusions.


Technical Support  
-----------------
Telephone support is available Monday through Friday from 7 a.m. 
to 5 p.m. PST at (510)661-3000.  Additional software drivers and 
upgrades are available through Orchid's 24-hour Bulletin Board 
Service (510)683-0327 (14.4K baud, 8N1).  Access Orchid support 
via our CompuServe forum.  Enter GO ORCHID at any ! prompt to 
enter the Orchid section of the Multimedia B Vendor Forum.


Orchid Technology                  Orchid Technology        
Technical Support                  Headquarters
232 East Warren Avenue             45365 Northport Loop West
Fremont, CA 94539-7085             Fremont, CA 94538
(510)661-3000                      (510)683-0300


Orchid France S.A.R.L.   Orchid Technology GmbH   Orchid (Europe) Ltd.
Colombes, France         Meerbusch, Germany       Basingstoke, UK
Tel:(33)-1-47 80 70 50   Tel:49 2132 80071        Tel: 256-479898

-- documentation revised 08/95  Orchid Technology Technical Support
