README.1ST

Tseng ET6000 Display Driver for OS/2

This readme file contains information on how to install the Tseng ET6000
Display Driver for OS/2


This OS/2 driver supports adaptors and system boards that use the ET6000
graphics controller.


README.1ST CONTENTS:

1.0 SYSTEM REQUIREMENTS
2.0 PRELIMINARY STEPS
3.0 INSTALLATION
4.0 PROBLEM DETERMINATION & TECHNICAL SUPPORT 
5.0 Tseng ET6000 Display Driver CONTENTS.
6.0 TRADEMARKS

1.0 System Requirements

Before you install the Tseng ET6000 Display Driver for OS/2, make sure that 
	you have:

	1) Installed OS/2 WARP Version 3.00 or above
	2) 8_MB of system memory
	3) 2_MB of hard disk space on your Boot Drive
	4) PKUNZIP.EXE (either OS/2 or DOS version)



2.0 PRELIMINARY STEPS

	1) Unzip the file OS2ET6.ZIP into a temporary directory on your
	   hard disk in order to get the following files:
		ET6000.ZIP (driver ZIP file)
		README.TXT (installation instructions)
		README.1ST (this file)

	2) Change to the temporary directory and make the Tseng ET6000
	   Display Driver for OS/2 install diskette by running:

	   [d:path] PKUNZIP -d ET6000 [d:]

		(where [d:path] is the drive and directory where your PKUNZIP
		 file resides, and [d:] is the drive that will contain
		 the install diskette.)

	 Example: C:\ZIP\PKUNZIP -d ET6000 A:

3.0 INSTALLATION

	1) Ensure all preliminary steps are completed from section 2.0 above.

	2) Complete installation instructions are in the README.TXT file.


4.0 Problem Determination & Technical Support

	1) To report a problem or obtain the latest release of Tseng ET6000
	   Display Driver for OS/2, you may contact Tseng Labs by the following
	   means:

		CompuServe - "GO TSENG"
		WWW site - "WWW.TSENG.COM"
	
5.0  TRADEMARKS

ET6000 is a trademark of Tseng Labs Inc. in the United States and/or
other countries.

The following terms, denoted by an asterisk (*) in this file, are trademarks 
or registered trademarks of IBM Corporation in the United States and/or other 
countries:

IBM
OS/2

